{"text_format":"1","workbook":"xlsx","n_sheets":12,"sheets":["Cover","BitMap","Data Memory Map","Change_log","ConstantValue","CHNOutput","HB_TURN_DPL_SBL","FAN","BIN","NTC_Derating","Animation","LEDFailure"],"not_rendered":{"charts":4,"images":2,"macros":1,"external_links":1,"defined_names":65,"comments":7,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":13,"n_cols":7,"rows_kept":13,"cut":false,"hidden":false,"merged":[[12,0,12,1],[5,0,5,2],[8,1,8,2],[9,0,9,2],[10,0,10,2],[11,0,11,1]]}
[]
[null,null,null,null,"Don't Change",null,"Automatic Generation"]
[null,null,null,null,"Fill In",null,"Error Entry"]
[]
[]
["General Information"]
["DataSet Version","A","B"]
["Project Version\n","DVX1","17"]
["Config Match\n",0]
["Generated Parameter String："]
["004D7E1045C28BA89EFD94880280000000000000088C20080200000800012D2D2D2D2D2D2D008C8C8C8C8C8C8C800404040404040430005050505050505BC0800357520006AEA6000D5D50001ABA996723EBE800000000000000000000001111124FD272"]
["0000000001001101011111100001000001000101110000101000101110101000100111101111110110010100100010000000001010000000000000000000000000000000000000000000000000000000000010001000110000100000000010000000001000000000000000000000100000000000000000010010110100101101001011010010110100101101001011010010110100000000100011001000110010001100100011001000110010001100100011001000000000000100000001000000010000000100000001000000010000000100001100000000000001010000010100000101000001010000010100000101000001011011110000001000000000000011010101110101001000000000000001101010111010100110000000000000110101011101010100000000000000011010101110101001100101100111001000111110101111101000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000010001000100010001001001001",null,{"$f":"LEN(A12)","v":781}]
["0000000001001101011111100001000001000101110000",null,{"$f":"LEN(A13)","v":46}]

{"sheet":"BitMap","index":1,"n_rows":101,"n_cols":33,"rows_kept":101,"cut":false,"hidden":true,"merged":[[81,32,96,32],[1,32,16,32],[17,32,32,32],[33,32,48,32],[49,32,64,32],[65,32,80,32]]}
["7","6","5","4","3","2","1","0","7","6","5","4","3","2","1","0","7","6","5","4","3","2","1","0","7","6","5","4","3","2","1","0"]
["0",null,null,null,null,null,null,null,"1",null,null,null,null,null,null,null,"2",null,null,null,null,null,null,null,"3",null,null,null,null,null,null,null,"1"]
["Basic_cfg"]
["Dataset_Version",null,null,null,null,null,null,null,null,null,"Project_Num"]
["Version_High",null,null,null,null,"Version_Low",null,null,null,null,"Project_Num1",null,null,null,null,null,"Project_Num2",null,null,null,null,null,"Project_Num3",null,null,null,null,null,"Project_Num4"]
["4",null,null,null,null,null,null,null,"5",null,null,null,null,null,null,null,"6",null,null,null,null,null,null,null,"7"]
["Basic_cfg",null,null,null,null,null,null,null,null,null,null,null,null,null,"CHNOutput"]
["Project_Num",null,null,null,null,null,null,null,null,null,"Config_Match",null,null,null,"Vf_Max_Voltage",null,null,null,"Output_CHN1",null,null,null,null,null,null,"Output_CHN2"]
["Project_Num4",null,"Project_Num5",null,null,null,"Project_Num6",null,null,null,"Config_Match",null,null,null,"Vf_Max_Voltage",null,null,null,"Usage",null,null,"LED_Num",null,null,null,"Usage",null,null,"LED_Num"]
["8",null,null,null,null,null,null,null,"9",null,null,null,null,null,null,null,"10",null,null,null,null,null,null,null,"11"]
["CHNOutput"]
["Output_CHN3",null,null,null,null,null,null,"Output_CHN4",null,null,null,null,null,null,"Output_LSD1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Output_LSD2"]
["Usage",null,null,"LED_Num",null,null,null,"Usage",null,null,"LED_Num",null,null,null,"Usage",null,null,"DutyCycle",null,null,null,null,null,null,"Assign_CHN",null,null,"LED_Num",null,null,null,"Usage"]
["12",null,null,null,null,null,null,null,"13",null,null,null,null,null,null,null,"14",null,null,null,null,null,null,null,"15"]
["CHNOutput"]
["Output_LSD2",null,null,null,null,null,null,"Output_LSD2",null,null,null,null,null,null,null,null,"Output_PWM1",null,null,null,null,null,null,null,null,null,null,"Output_PWM2"]
["Usage",null,"DutyCycle",null,null,null,null,"DutyCycle",null,"Assign_CHN",null,null,"LED_Num",null,null,null,"Usage",null,null,null,"DutyCycle",null,null,null,null,null,null,"Usage",null,null,null,"DutyCycle"]
["16",null,null,null,null,null,null,null,"17",null,null,null,null,null,null,null,"18",null,null,null,null,null,null,null,"19",null,null,null,null,null,null,null,"2"]
["CHNOutput",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LampCfg"]
["Output_PWM2",null,null,null,null,null,"Output_PWM3",null,null,null,null,null,null,null,null,null,null,"Output_PWM4",null,null,null,null,null,null,null,null,null,null,"HB_CFG"]
["DutyCycle",null,null,null,null,null,"Usage",null,null,null,"DutyCycle",null,null,null,null,null,null,"Usage",null,null,null,"DutyCycle",null,null,null,null,null,null,"Ramp_Method","Combine_Fog",null,"LDM_Ramp"]
["20",null,null,null,null,null,null,null,"21",null,null,null,null,null,null,null,"22",null,null,null,null,null,null,null,"23"]
["LampCfg"]
["HB_CFG",null,null,null,null,null,null,null,null,null,null,null,null,"TURN_CFG",null,null,null,null,"DPL_CFG"]
["LDM_Ramp","Fade_Fast",null,null,null,"Fade_Mid",null,null,null,"Fade_Slow",null,null,null,"Signal_Source","Delay_Time",null,null,null,"Signal_Source",null,"PL_Trigger_DutyCycle",null,null,null,null,"PL_DutyCycle",null,null,null,null,null,"Combine_LB_Outage"]
["24",null,null,null,null,null,null,null,"25",null,null,null,null,null,null,null,"26",null,null,null,null,null,null,null,"27"]
["LampCfg",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FAN"]
["DPL_CFG",null,null,null,null,null,null,null,null,"SBL_CFG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FAN_CFG"]
["Combine_LB_Outage","DRL_Combine_TI","DRL_TI_Control",null,"DRL_Activation_Time_After_Deact",null,null,null,"DRL_ON_FTP","Trigger_SteerAngle",null,null,null,null,null,null,null,"MAX_Speed",null,null,null,null,null,null,null,"SelftestTime",null,"Outage_Detect","Active_Condition",null,"Assign_NTC"]
["28",null,null,null,null,null,null,null,"29",null,null,null,null,null,null,null,"30",null,null,null,null,null,null,null,"31"]
["FAN",null,null,null,"BIN"]
["FAN_CFG",null,null,null,"CHN1_BIN_CFG"]
["Active_Temp",null,null,null,"BIN_Source",null,"BIN_Para",null,null,null,null,null,null,null,"BIN1_Current",null,null,null,null,null,null,null,"BIN2_Current",null,null,null,null,null,null,null,"BIN3_Current"]
["32",null,null,null,null,null,null,null,"33",null,null,null,null,null,null,null,"34",null,null,null,null,null,null,null,"35",null,null,null,null,null,null,null,"3"]
["BIN"]
["CHN1_BIN_CFG"]
["BIN3_Current",null,null,null,null,null,"BIN4_Current",null,null,null,null,null,null,null,"BIN5_Current",null,null,null,null,null,null,null,"BIN6_Current",null,null,null,null,null,null,null,"BIN7_Current"]
["36",null,null,null,null,null,null,null,"37",null,null,null,null,null,null,null,"38",null,null,null,null,null,null,null,"39"]
["BIN"]
["CHN1_BIN_CFG",null,null,null,null,null,"CHN2_BIN_CFG"]
["BIN7_Current",null,null,null,null,null,"BIN_Source",null,"BIN_Para",null,null,null,null,null,null,null,"BIN1_Current",null,null,null,null,null,null,null,"BIN2_Current"]
["40",null,null,null,null,null,null,null,"41",null,null,null,null,null,null,null,"42",null,null,null,null,null,null,null,"43"]
["BIN"]
["CHN2_BIN_CFG"]
["BIN3_Current",null,null,null,null,null,null,null,"BIN4_Current",null,null,null,null,null,null,null,"BIN5_Current",null,null,null,null,null,null,null,"BIN6_Current"]
["44",null,null,null,null,null,null,null,"45",null,null,null,null,null,null,null,"46",null,null,null,null,null,null,null,"47"]
["BIN"]
["CHN2_BIN_CFG",null,null,null,null,null,null,null,"CHN3_BIN_CFG"]
["BIN7_Current",null,null,null,null,null,null,null,"BIN_Source",null,"BIN_Para",null,null,null,null,null,null,null,"BIN1_Current",null,null,null,null,null,null,null,"BIN2_Current"]
["48",null,null,null,null,null,null,null,"49",null,null,null,null,null,null,null,"50",null,null,null,null,null,null,null,"51",null,null,null,null,null,null,null,"4"]
["BIN"]
["CHN3_BIN_CFG"]
["BIN2_Current",null,"BIN3_Current",null,null,null,null,null,null,null,"BIN4_Current",null,null,null,"BIN4_Current",null,null,null,"BIN5_Current",null,null,null,null,null,null,null,"BIN6_Current"]
["52",null,null,null,null,null,null,null,"53",null,null,null,null,null,null,null,"54",null,null,null,null,null,null,null,"55"]
["BIN"]
["CHN3_BIN_CFG",null,null,null,null,null,null,null,null,null,"CHN4_BIN_CFG"]
["BIN6_Current",null,"BIN7_Current",null,null,null,null,null,null,null,"BIN_Source",null,"BIN_Para",null,null,null,null,null,null,null,"BIN1_Current",null,null,null,null,null,null,null,"BIN2_Current"]
["56",null,null,null,null,null,null,null,"57",null,null,null,null,null,null,null,"58",null,null,null,null,null,null,null,"59"]
["BIN"]
["CHN4_BIN_CFG"]
["BIN2_Current",null,null,null,"BIN3_Current",null,null,null,null,null,null,null,"BIN4_Current",null,null,null,null,null,null,null,"BIN5_Current",null,null,null,null,null,null,null,"BIN6_Current"]
["60",null,null,null,null,null,null,null,"61",null,null,null,null,null,null,null,"62",null,null,null,null,null,null,null,"63"]
["BIN",null,null,null,null,null,null,null,null,null,null,null,"NTC"]
["CHN4_BIN_CFG",null,null,null,null,null,null,null,null,null,null,null,"NTC_CFG",null,null,null,null,null,null,null,null,null,"CHN1_NTC_CFG"]
["BIN6_Current",null,null,null,"BIN7_Current",null,null,null,null,null,null,null,"R0","B_Constant",null,null,null,null,null,null,null,null,"NTC_Source",null,null,"Derate1_Dim",null,"Derate2_Temp",null,null,"Derate2_Dim"]
["64",null,null,null,null,null,null,null,"65",null,null,null,null,null,null,null,"66",null,null,null,null,null,null,null,"67",null,null,null,null,null,null,null,"5"]
["NTC"]
["CHN1_NTC_CFG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CHN2_NTC_CFG"]
["Derate3_Temp",null,null,"Derate3_Dim",null,null,"Derate4_Temp",null,null,"Derate4_Dim",null,null,null,"Derate5_Temp",null,null,"Derate5_Dim",null,null,null,null,"NTC_Source",null,null,"Derate1_Dim",null,"Derate2_Temp",null,null,"Derate2_Dim",null,"Derate3_Temp"]
["68",null,null,null,null,null,null,null,"69",null,null,null,null,null,null,null,"70",null,null,null,null,null,null,null,"71"]
["NTC"]
["CHN2_NTC_CFG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CHN3_NTC_CFG"]
["Derate3_Temp",null,"Derate3_Dim",null,null,"Derate4_Temp",null,null,"Derate4_Dim",null,null,null,"Derate5_Temp",null,null,"Derate5_Dim",null,null,null,null,"NTC_Source",null,null,"Derate1_Dim",null,"Derate2_Temp",null,null,"Derate2_Dim",null,"Derate3_Temp"]
["72",null,null,null,null,null,null,null,"73",null,null,null,null,null,null,null,"74",null,null,null,null,null,null,null,"75"]
["NTC"]
["CHN3_NTC_CFG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CHN4_NTC_CFG"]
["Derate3_Temp","Derate3_Dim",null,null,"Derate4_Temp",null,null,"Derate4_Dim",null,null,null,"Derate5_Temp",null,null,"Derate5_Dim",null,null,null,null,"NTC_Source",null,null,"Derate1_Dim",null,"Derate2_Temp",null,null,"Derate2_Dim",null,"Derate3_Temp"]
["76",null,null,null,null,null,null,null,"77",null,null,null,null,null,null,null,"78",null,null,null,null,null,null,null,"79"]
["NTC",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ANIM"]
["CHN4_NTC_CFG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ANIM_CFG",null,null,null,null,null,null,null,null,null,null,null,"DRL_ANIM_CFG"]
["Derate3_Dim",null,null,"Derate4_Temp",null,null,"Derate4_Dim",null,null,null,"Derate5_Temp",null,null,"Derate5_Dim",null,null,null,null,"Welcome_Delay",null,null,null,null,null,"Farewell_Delay",null,null,null,null,null,"Target_DutyCycle"]
["80",null,null,null,null,null,null,null,"81",null,null,null,null,null,null,null,"82",null,null,null,null,null,null,null,"83",null,null,null,null,null,null,null,"6"]
["ANIM"]
["DRL_ANIM_CFG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PWM1_ANIM_CFG"]
["Target_DutyCycle",null,null,null,null,"Fade_On_Duration",null,null,null,null,null,null,null,"Fade_Off_Duration",null,null,null,null,null,null,null,"Target_DutyCycle",null,null,null,null,null,null,"Fade_On_Duration"]
["84",null,null,null,null,null,null,null,"85",null,null,null,null,null,null,null,"86",null,null,null,null,null,null,null,"87"]
["ANIM"]
["PWM1_ANIM_CFG",null,null,null,"PWM1_ANIM_CFG",null,null,null,null,null,null,null,"PWM2_ANIM_CFG"]
["Fade_On_Duration",null,null,null,"Fade_Off_Duration",null,null,null,null,null,null,null,"Target_DutyCycle",null,null,null,null,null,null,"Fade_On_Duration",null,null,null,null,null,null,null,"Fade_Off_Duration"]
["88",null,null,null,null,null,null,null,"89",null,null,null,null,null,null,null,"90",null,null,null,null,null,null,null,"91"]
["ANIM"]
["PWM2_ANIM_CFG",null,null,"PWM3_ANIM_CFG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"PWM4_ANIM_CFG"]
["Fade_Off_Duration",null,null,"Target_DutyCycle",null,null,null,null,null,null,"Fade_On_Duration",null,null,null,null,null,null,null,"Fade_Off_Duration",null,null,null,null,null,null,null,"Target_DutyCycle"]
["92",null,null,null,null,null,null,null,"93",null,null,null,null,null,null,null,"94",null,null,null,null,null,null,null,"95"]
["ANIM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LEDFailure"]
["PWM4_ANIM_CFG",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CHN_Fault_CFG"]
["Target_DutyCycle","Fade_On_Duration",null,null,null,null,null,null,null,"Fade_Off_Duration",null,null,null,null,null,null,null,"CHN1_Single_LED_Vf",null,null,null,"CHN2_Single_LED_Vf",null,null,null,"CHN3_Single_LED_Vf",null,null,null,"CHN4_Single_LED_Vf"]
["96",null,null,null,null,null,null,null,"97",null,null,null,null,null,null,null,"98",null,null,null,null,null,null,null,"99"]
["LEDFailure",null,null,null,null,null,null,null,null,null,null,null,null,"补位",null,null,"CRC"]
["CHN_Fault_CFG","LB_Fault_CFG",null,null,"HB_Fault_CFG",null,null,"DRL_Fault_CFG",null,null,"TI_Fault_CFG",null,null,"Aligning"]
["CHN4_Single_LED_Vf","Fault_Deact",null,"Falut_Report","Fault_Deact",null,"Falut_Report","Fault_Deact",null,"Falut_Report","Fault_Deact",null,"Falut_Report","Aligning"]

{"sheet":"Data Memory Map","index":2,"n_rows":13,"n_cols":20,"rows_kept":13,"cut":false,"hidden":true,"merged":[]}
[]
[]
[]
[]
[]
[null,null,null,null,"0","1","2","3","4","5","6","7","8","9","A","B","C","D","E","F"]
[null,null,null,null,"00","61","39","85","41","42","8F","9F","82","C4","B2","2C","59","26","1C","83"]
[null,null,null,null,"90","72","0E","40","08","8C","12","E2","02","00","00","18","00","00","A0","A0"]
[null,null,null,null,"A0","A0","A0","A0","A1","00","05","05","05","05","05","05","05","80","23","23"]
[null,null,null,null,"23","23","23","23","23","30","08","C8","C8","C8","C8","C8","C8","C4","10","80"]
[null,null,null,null,"22","04","61","00","44","08","C0","00","00","00","00","00","00","00","01","07"]
[null,null,null,null,"22","5A","58","00","00","00","00","00","00","00","00","00","00","00","11","11"]
[null,null,null,null,"12","4F","86","30"]

{"sheet":"Change_log","index":3,"n_rows":27,"n_cols":5,"rows_kept":27,"cut":false,"hidden":true,"merged":[]}
["APP Version","Version","Data","Comments","Author"]
["NA","AA.1","2024-06-12","Initial Version","Peiyuan Zuo"]
["NA","AA.2","2024-06-25","Complete Part \"CHNOutput\"","Peiyuan Zuo"]
["NA","AA.3","2024-07-01","Complete Part \"HB_TURN_DPL_SBL\"and\"FAN\"","Peiyuan Zuo"]
["NA","AA.4","2024-07-04","Complete Part \"BIN\",\"NTC_Derating\",\"Animation\"，\"LEDFailure\" , Bit→HEX and CRC","Peiyuan Zuo"]
["NA","AA.5","2024-07-05","Update BitMap","Peiyuan Zuo"]
["NA","AA.6","2024-07-11","Corrected version number generated","Peiyuan Zuo"]
["NA","AA.6.1","2024-07-12","Change the data structure description","Peiyuan Zuo"]
["NA","AA.7","2024-07-11","Added table protection against illegal modifications","Peiyuan Zuo"]
["NA","AA.7.1","2024-07-15","Change the data structure description","Peiyuan Zuo"]
["NA","AA.7.2","2024-07-25","Change the data structure description\nAdd the \"Project Version\"","Peiyuan Zuo"]
["NA","AA.7.3","2024-08-16","Change according to customer requirements","Peiyuan Zuo"]
["NA","AA.7.4","2024-08-20","Change bitmap","Peiyuan Zuo"]
["NA","AA.7.5","2024-08-20","Integrate interface code generation capabilities","Peiyuan Zuo"]
["NA","AA.7.6","2024-08-22","Change bitmap to provide software validation","Peiyuan Zuo"]
["NA","AA.7.7","2024-08-22","Configure the 764 project base items\nChange the bitmap calculation script","Peiyuan Zuo"]
["SW0007169.A001","AA.7.8","2024-08-23","The linkage between fault detection and reporting is cancelled","Peiyuan Zuo"]
["SW0007169.A001","AA.7.9","2024-08-29","Change the data structure for Animation and LEDFailure","Peiyuan Zuo"]
["SW0007169.A001","AA.7.10","2024-09-06","Change the Value change for \"DRL_Combined_TI\" and \"Config Match\"","Peiyuan Zuo"]
["SW0007169.A001","AA","2024-10-08","Fixed an issue where customer's computer was not running","Peiyuan Zuo"]
["SW0007169.A001.6","AA.7.11","2024-10-09","1. If lb does not detect faults, the \"DRL_LB_Outage\" option is disabled\n2.Added LSD \"Not_Used\" linkage and Modify the low side duty cycle range\n3.The bin current is changed to 100 mA to 1500 mAand can be entered manually\n4.Change the Options of  \"DRL_Combined_TI\" and \"DRL_TI_Control\"\n5.FAN linkage problems are modified\n6.Optimize the interface and add parameter remarks","Peiyuan Zuo"]
["SW0007169.A001.6","AA.7.12","2024-10-12","Correct the option name of DRL_TI_Control","Peiyuan Zuo"]
["SW0007169.A001.6","AA.7.13","2024-10-13","Update the generated para raw data to meet QAC test","Shengwei Zhu"]
["SW0007169.A001.6","AB","2024-10-17","Solution When DRL2 exists, \"TI_active,turnoff_DRL2,no_impact_on_PO2/DRL1/PO1\" cannot be selected from \"DRL_TI_Control\"\nOfficial release","Peiyuan Zuo"]
["SW0007169.A001.8","AB.1","2024-11-01","1.Added anti-dork Settings for DRL/PO functions\n2.The bin0 value of BIN Para cfg is set to the low value\n3.Open the duty cycle setting of the DRL1/2 corresponding to the PWM channel\n4.Update NTC Derate5 options range\n5.Corrected NTC verification function\n","Peiyuan Zuo"]
["SW0007169.A001.8","AB.2","2024-11-04","Modify the comment for W/F_Delay_cfg","Peiyuan Zuo"]
["SW0007169.A001.8","AB.3","2024-11-04","Modify the range and data size of NTC Derate5 Dimming cfg","Peiyuan Zuo"]

{"sheet":"ConstantValue","index":4,"n_rows":176,"n_cols":347,"rows_kept":176,"cut":false,"hidden":true,"merged":[[162,4,163,4],[165,4,166,4],[168,4,169,4],[171,4,172,4],[0,0,2,1],[147,4,148,4],[150,4,151,4],[153,4,154,4],[156,4,157,4],[159,4,160,4],[132,4,133,4],[135,4,136,4],[138,4,139,4],[141,4,142,4],[144,4,145,4],[117,4,118,4],[120,4,121,4],[123,4,124,4],[126,4,127,4],[129,4,130,4],[102,4,103,4],[105,4,106,4],[108,4,109,4],[111,4,112,4],[114,4,115,4],[87,4,88,4],[90,4,91,4],[93,4,94,4],[96,4,97,4],[99,4,100,4],[72,4,73,4],[75,4,76,4],[78,4,79,4],[81,4,82,4],[84,4,85,4],[57,4,58,4],[60,4,61,4],[63,4,64,4],[66,4,67,4],[69,4,70,4],[42,4,43,4],[45,4,46,4],[48,4,49,4],[51,4,52,4],[54,4,55,4],[114,3,148,3],[150,3,163,3],[165,3,172,3],[3,4,4,4],[6,4,7,4],[9,4,10,4],[12,4,13,4],[15,4,16,4],[18,4,19,4],[21,4,22,4],[24,4,25,4],[27,4,28,4],[30,4,31,4],[33,4,34,4],[36,4,37,4],[39,4,40,4],[3,3,13,3],[15,3,37,3],[39,3,88,3],[90,3,103,3],[105,3,112,3],[174,0,175,0],[0,2,2,2],[3,2,13,2],[15,2,37,2],[39,2,88,2],[90,2,103,2],[105,2,112,2],[114,2,148,2],[150,2,163,2],[165,2,172,2]]}
["数据大小（bits）",null,"total（bits)"]
[]
[]
["2x5bits",10,{"$f":"SUM(B4:B14)","v":46},"Cover","DateSheet_Version","A","B","C","D","E","F","G","H","I","J","K","L","M","N","O","P","Q","R","S","T","U","V","W","X","Y","Z"]
[null,null,null,null,null,0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25]
[]
["4x6bits",24,null,null,"Project_Num",0,1,2,3,4,5,6,7,8,9,"A","B","C","D","E","F","G","H","I","J","K","L","M","N","O","P","Q","R","S","T","U","V","W","X","Y","Z"]
[null,null,null,null,null,0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26,27,28,29,30,31,32,33,34,35]
[]
["2x4bits",8,null,null,"Project_Version",0,1,2,3,4,5,6,7,8,9]
[null,null,null,null,null,0,1,2,3,4,5,6,7,8,9]
[]
["4bits",4,null,null,"Config_Match",0,1,2,3,4,5,6,7,8,9,"A","B","C","D","E","F"]
[null,null,null,null,null,0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15]
[]
["4x3bits",12,{"$f":"SUM(B16:B38)","v":110},"CHNOutput","Channel_usage","Not_Used","LB","HB","DRL","TI"]
[null,null,null,null,null,0,1,2,3,4,7]
[]
["2x3bits",6,null,null,"LSD_channel_assignment","Not_Used","Channel1","Channel2","Channel3","Channel4"]
[null,null,null,null,null,0,1,2,3,4,7]
[]
["2x3bits",6,null,null,"LSD_usage","Not_Used","LB","HB","DRL2","SBL"]
[null,null,null,null,null,0,1,2,3,4,5,6,7]
[]
["2x7bits",14,null,null,"LSD_Duty_Cycle"]
[null,null,null,null,null,127]
[]
[null,4,null,null,"Vf_Maximum_voltage",0,5,10,15,20,25,30,35,40,45,50]
[null,null,null,null,null,0,1,2,3,4,5,6,7,8,9,10,15]
[]
["4x4bits",16,null,null,"PWM_Function_Assign","Not_Used","LB","HB","TI/Hazard","DRL1","DRL2","Licoln_Lit_Star","Front_Fog","Cornering","SideMarker","StaticBending"]
[null,null,null,null,null,0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15]
[]
["4x7bits",28,null,null,"PWM_Target_Duty_Cycle"]
[null,null,null,null,null,127]
[]
["6x4bits",24,null,null,"Num_LED","Not_Used",1,2,3,4,5,6,7,8,9,10,11,12,13,14,15]
[null,null,null,null,null,0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15]
[]
[null,1,{"$f":"SUM(B40:B89)","v":61},"LampCfg","HB_Ramp_method","BCM_LIN","LDM"]
[null,null,null,null,null,0,1]
[]
["3x4bits",12,null,null,"HB_fade_spd",100,200,300,400,500,600,800,1000,1250,1500,1750,2000,2500,3000,3500,4000]
[null,null,null,null,null,0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15]
[]
[null,2,null,null,"LDM_internal_standard_ramping","Immediate","Fade_In100ms","Fade_In150ms","Fade_In200ms"]
[null,null,null,null,null,0,1,2,3]
[]
[null,2,null,null,"HB&Front_fog","INVALID","Fade_In100ms","Fade_In150ms","Fade_In200ms"]
[null,null,null,null,null,0,1,2,3]
[]
[null,null,null,null,"二级联动","BCM_LIN","Immediate"]
[null,null,null,null,null,"LDM","Immediate","Fade_In100ms","Fade_In150ms","Fade_In200ms"]
[]
[null,4,null,null,"TI_delay_time",0,30,60,90,120,150,180,210,240,270,300]
[null,null,null,null,null,0,1,2,3,4,5,6,7,8,9,10,15]
[]
[null,1,null,null,"TI_Signal_Source","INVALID","InputCHN3"]
[null,null,null,null,null,0,1]
[]
[null,2,null,null,"DRL_Signal_Source","INVALID","InputCHN4","BCM_LIN"]
[null,null,null,null,null,0,1,2,3]
[]
[null,5,null,null,"DPL_Trigger_Dutycycle","10","11","12","13","14","15","16","17","18","19","20","21","22","23","24","25","26","27","28","29","30","31","32","33","34","35","36","37","38","39","40","41"]
[null,null,null,null,null,0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26,27,28,29,30,31]
[]
[null,6,null,null,"ParkPos_Intensity","1","2","3","4","5","6","7","8","9","10","11","12","13","14","15","16","17","18","19","20","21","22","23","24","25","26","27","28","29","30","31","32","33","34","35","36","37","38","39","40","41","42","43","44","45","46","47","48","49","50"]
[null,null,null,null,null,0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26,27,28,29,30,31,32,33,34,35,36,37,38,39,40,41,42,43,44,45,46,47,48,49,63]
[]
[null,2,null,null,"DPL_LB_Outage","No_Impact","DRLtoPL_PLkeep","DRLkeep_PLOFF"]
[null,null,null,null,null,0,1,2,3]
[]
[null,1,null,null,"DRL_Combined_TI","TI_restrain_DRL/PO","TI_interact_with_DRL/PO"]
[null,null,null,null,null,0,1]
[]
[null,2,null,null,"DRL_TI_Control","TI_ON,DRL1Off/TI_OFF,DRL1ON","TI_ON,DRL1toPL1/TI_OFF,PL1toDRL1","TI_has_no_impact_on_DRL1/PO1","TI_active,turn_off_DRL1/PO1","TI_active,dim_DRL1toPO1","TI_active,turn_off_DRL1,no_impact_on","TI_active,turnoff_DRL1/2orPO2,no_impact_on_PO1","TI_active,turnoff_DRL2orPO2,no_impact_on_DRL1orPO1","TI_active,dim_DRL2toPO2,no_impact_on_DRL1orPO1","TI_active,turnoff_DRL2,no_impact_on_PO2/DRL1/PO1"]
[null,null,null,null,null,0,1,0,1,2,3,0,1,2,3]
[]
[null,4,null,null,"DRL_activation_time_after_deact",0,100,200,300,400,500,600,700,800,900,1000]
[null,null,null,null,null,0,1,2,3,4,5,6,7,8,9,10,15]
[]
[null,1,null,null,"DRL_ON_FTP","No_Impact","DRL_to_PL"]
[null,null,null,null,null,0,1]
[]
[null,8,null,null,"SBL_Trigger_SteAngle_Thershold"]
[]
[]
[null,8,null,null,"SBL_Max_Speed_Thershold"]
[]
[]
[null,2,{"$f":"SUM(B91:B104)","v":11},"FAN","FanRunTime_OnPwr",0,20,40,60]
[null,null,null,null,null,0,1,2,3]
[]
[null,2,null,null,"FAN_Activation_Trigger","No_Fan","Ignition_On","LB/HB_Active","Over_set_temp"]
[null,null,null,null,null,0,1,2,3]
[]
[null,2,null,null,"FAN_Activation_NTC","NTC1","NTC2","NTC3","NTC4"]
[null,null,null,null,null,0,1,2,3]
[]
[null,4,null,null,"Fan_Activation_Temp",50,55,60,65,70,75,80,85,90,95,100]
[null,null,null,null,null,0,1,2,3,4,5,6,7,8,9,10,15]
[]
[null,1,null,null,"Fan_Outage_Detect","DISABLE","ENABLE"]
[null,null,null,null,null,0,1]
[]
["4X8X1bit",32,{"$f":"SUM(B106:B113)","v":264},"BIN","BIN_Param_Cfg",0,1]
[null,null,null,null,null,0,1]
[]
["4x2bits",8,null,null,"Channel_BIN_Source","BIN_Channel1","BIN_Channel2","BIN_Channel3","BIN_Channel4"]
[null,null,null,null,null,0,1,2,3]
[]
["4x7x8bits",224,null,null,"CHN_Current",100,110,120,130,140,150,160,170,180,190,200,210,220,230,240,250,260,270,280,290,300,310,320,330,340,350,360,370,380,390,400,410,420,430,440,450,460,470,480,490,500,510,520,530,540,550,560,570,580,590,600,610,620,630,640,650,660,670,680,690,700,710,720,730,740,750,760,770,780,790,800,810,820,830,840,850,860,870,880,890,900,910,920,930,940,950,960,970,980,990,1000,1010,1020,1030,1040,1050,1060,1070,1080,1090,1100,1110,1120,1130,1140,1150,1160,1170,1180,1190,1200,1210,1220,1230,1240,1250,1260,1270,1280,1290,1300,1310,1320,1330,1340,1350,1360,1370,1380,1390,1400,1410,1420,1430,1440,1450,1460,1470,1480,1490,1500]
[null,null,null,null,null,0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26,27,28,29,30,31,32,33,34,35,36,37,38,39,40,41,42,43,44,45,46,47,48,49,50,51,52,53,54,55,56,57,58,59,60,61,62,63,64,65,66,67,68,69,70,71,72,73,74,75,76,77,78,79,80,81,82,83,84,85,86,87,88,89,90,91,92,93,94,95,96,97,98,99,100,101,102,103,104,105,106,107,108,109,110,111,112,113,114,115,116,117,118,119,120,121,122,123,124,125,126,127,128,129,130,131,132,133,134,135,136,137,138,139,140]
[]
[null,1,{"$f":"SUM(B115:B149)","v":134},"NTC","NTC_R0",47,10]
[null,null,null,null,null,0,1]
[]
[null,9,null,null,"NTC_B_Constant",2800,2805,2810,2815,2820,2825,2830,2835,2840,2845,2850,2855,2860,2865,2870,2875,2880,2885,2890,2895,2900,2905,2910,2915,2920,2925,2930,2935,2940,2945,2950,2955,2960,2965,2970,2975,2980,2985,2990,2995,3000,3005,3010,3015,3020,3025,3030,3035,3040,3045,3050,3055,3060,3065,3070,3075,3080,3085,3090,3095,3100,3105,3110,3115,3120,3125,3130,3135,3140,3145,3150,3155,3160,3165,3170,3175,3180,3185,3190,3195,3200,3205,3210,3215,3220,3225,3230,3235,3240,3245,3250,3255,3260,3265,3270,3275,3280,3285,3290,3295,3300,3305,3310,3315,3320,3325,3330,3335,3340,3345,3350,3355,3360,3365,3370,3375,3380,3385,3390,3395,3400,3405,3410,3415,3420,3425,3430,3435,3440,3445,3450,3455,3460,3465,3470,3475,3480,3485,3490,3495,3500,3505,3510,3515,3520,3525,3530,3535,3540,3545,3550,3555,3560,3565,3570,3575,3580,3585,3590,3595,3600,3605,3610,3615,3620,3625,3630,3635,3640,3645,3650,3655,3660,3665,3670,3675,3680,3685,3690,3695,3700,3705,3710,3715,3720,3725,3730,3735,3740,3745,3750,3755,3760,3765,3770,3775,3780,3785,3790,3795,3800,3805,3810,3815,3820,3825,3830,3835,3840,3845,3850,3855,3860,3865,3870,3875,3880,3885,3890,3895,3900,3905,3910,3915,3920,3925,3930,3935,3940,3945,3950,3955,3960,3965,3970,3975,3980,3985,3990,3995,4000,4005,4010,4015,4020,4025,4030,4035,4040,4045,4050,4055,4060,4065,4070,4075,4080,4085,4090,4095,4100,4105,4110,4115,4120,4125,4130,4135,4140,4145,4150,4155,4160,4165,4170,4175,4180,4185,4190,4195,4200,4205,4210,4215,4220,4225,4230,4235,4240,4245,4250,4255,4260,4265,4270,4275,4280,4285,4290,4295,4300,4305,4310,4315,4320,4325,4330,4335,4340,4345,4350,4355,4360,4365,4370,4375,4380,4385,4390,4395,4400,4405,4410,4415,4420,4425,4430,4435,4440,4445,4450,4455,4460,4465,4470,4475,4480,4485,4490,4495,4500]
[null,null,null,null,null,0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26,27,28,29,30,31,32,33,34,35,36,37,38,39,40,41,42,43,44,45,46,47,48,49,50,51,52,53,54,55,56,57,58,59,60,61,62,63,64,65,66,67,68,69,70,71,72,73,74,75,76,77,78,79,80,81,82,83,84,85,86,87,88,89,90,91,92,93,94,95,96,97,98,99,100,101,102,103,104,105,106,107,108,109,110,111,112,113,114,115,116,117,118,119,120,121,122,123,124,125,126,127,128,129,130,131,132,133,134,135,136,137,138,139,140,141,142,143,144,145,146,147,148,149,150,151,152,153,154,155,156,157,158,159,160,161,162,163,164,165,166,167,168,169,170,171,172,173,174,175,176,177,178,179,180,181,182,183,184,185,186,187,188,189,190,191,192,193,194,195,196,197,198,199,200,201,202,203,204,205,206,207,208,209,210,211,212,213,214,215,216,217,218,219,220,221,222,223,224,225,226,227,228,229,230,231,232,233,234,235,236,237,238,239,240,241,242,243,244,245,246,247,248,249,250,251,252,253,254,255,256,257,258,259,260,261,262,263,264,265,266,267,268,269,270,271,272,273,274,275,276,277,278,279,280,281,282,283,284,285,286,287,288,289,290,291,292,293,294,295,296,297,298,299,300,301,302,303,304,305,306,307,308,309,310,311,312,313,314,315,316,317,318,319,320,321,322,323,324,325,326,327,328,329,330,331,332,333,334,335,336,337,338,339,340,511]
[]
["4x3bits",12,null,null,"Channel_NTC_Source","Not_Used","NTC1","NTC2","NTC3","NTC4"]
[null,null,null,null,null,0,1,2,3,4,7]
[]
["4x3bits",12,null,null,"CHx_NTC_TempDerate2",-5,0,5,10,15,20,25,30]
[null,null,null,null,null,0,1,2,3,4,5,6,7]
[]
["4x3bits",12,null,null,"CHx_NTC_TempDerate3",80,85,90,95,100,105,110,115]
[null,null,null,null,null,0,1,2,3,4,5,6,7]
[]
["4x3bits",12,null,null,"CHx_NTC_TempDerate4",90,95,100,105,110,115,120,125]
[null,null,null,null,null,0,1,2,3,4,5,6,7]
[]
["4x3bits",12,null,null,"CHx_NTC_TempDerate5",100,105,110,115,120,125,130,135]
[null,null,null,null,null,0,1,2,3,4,5,6,7]
[]
["4x2bits",8,null,null,"CHx_NTC_BrightDerate1",0,5,10,15]
[null,null,null,null,null,0,1,2,3]
[]
["4x2bits",8,null,null,"CHx_NTC_BrightDerate2",0,5,10,15]
[null,null,null,null,null,0,1,2,3]
[]
["4x3bits",12,null,null,"CHx_NTC_BrightDerate3",0,5,10,15,20,25,30,35]
[null,null,null,null,null,0,1,2,3,4,5,6,7]
[]
["4x4bits",16,null,null,"CHx_NTC_BrightDerate4",0,5,10,15,20,25,30,35,40,45,50,55,60,65,70,75]
[null,null,null,null,null,0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15]
[]
["4x5bits",20,null,null,"CHx_NTC_BrightDerate5",0,5,10,15,20,25,30,35,40,45,50,55,60,65,70,75,80,85,90,95,100]
[null,null,null,null,null,0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,31]
[]
[null,7,{"$f":"SUM(B151:B164)","v":127},"Animation","DRL_Embrace_Intensity"]
[null,null,null,null,null,127]
[]
[null,16,null,null,"DRL_Curve_Duration_Welcome/Farewell",0,40,80,120,160,200,240,280,320,360,400,440,480,520,560,600,640,680,720,760,800,840,880,920,960,1000,1040,1080,1120,1160,1200,1240,1280,1320,1360,1400,1440,1480,1520,1560,1600,1640,1680,1720,1760,1800,1840,1880,1920,1960,2000,2040,2080,2120,2160,2200,2240,2280,2320,2360,2400,2440,2480,2520,2560,2600,2640,2680,2720,2760,2800,2840,2880,2920,2960,3000,3040,3080,3120,3160,3200,3240,3280,3320,3360,3400,3440,3480,3520,3560,3600,3640,3680,3720,3760,3800,3840,3880,3920,3960,4000,4040,4080,4120,4160,4200,4240,4280,4320,4360,4400,4440,4480,4520,4560,4600,4640,4680,4720,4760,4800,4840,4880,4920,4960,5000,5040,5080,5120,5160,5200,5240,5280,5320,5360,5400,5440,5480,5520,5560,5600,5640,5680,5720,5760,5800,5840,5880,5920,5960,6000,6040,6080,6120,6160,6200,6240,6280,6320,6360,6400,6440,6480,6520,6560,6600,6640,6680,6720,6760,6800,6840,6880,6920,6960,7000,7040,7080,7120,7160,7200,7240,7280,7320,7360,7400,7440,7480,7520,7560,7600,7640,7680,7720,7760,7800,7840,7880,7920,7960,8000,8040,8080,8120,8160,8200,8240,8280,8320,8360,8400,8440,8480,8520,8560,8600,8640,8680,8720,8760,8800,8840,8880,8920,8960,9000,9040,9080,9120,9160,9200,9240,9280,9320,9360,9400,9440,9480,9520,9560,9600,9640,9680,9720,9760,9800,9840,9880,9920,9960,10000]
[null,null,null,null,null,0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26,27,28,29,30,31,32,33,34,35,36,37,38,39,40,41,42,43,44,45,46,47,48,49,50,51,52,53,54,55,56,57,58,59,60,61,62,63,64,65,66,67,68,69,70,71,72,73,74,75,76,77,78,79,80,81,82,83,84,85,86,87,88,89,90,91,92,93,94,95,96,97,98,99,100,101,102,103,104,105,106,107,108,109,110,111,112,113,114,115,116,117,118,119,120,121,122,123,124,125,126,127,128,129,130,131,132,133,134,135,136,137,138,139,140,141,142,143,144,145,146,147,148,149,150,151,152,153,154,155,156,157,158,159,160,161,162,163,164,165,166,167,168,169,170,171,172,173,174,175,176,177,178,179,180,181,182,183,184,185,186,187,188,189,190,191,192,193,194,195,196,197,198,199,200,201,202,203,204,205,206,207,208,209,210,211,212,213,214,215,216,217,218,219,220,221,222,223,224,225,226,227,228,229,230,231,232,233,234,235,236,237,238,239,240,241,242,243,244,245,246,247,248,249,250,255]
[]
[null,12,null,null,"DRL_Embrace_Delay_Welcome/Farewell",0,40,80,120,160,200,240,280,320,360,400,440,480,520,560,600,640,680,720,760,800,840,880,920,960,1000,1040,1080,1120,1160,1200,1240,1280,1320,1360,1400,1440,1480,1520,1560,1600,1640,1680,1720,1760,1800,1840,1880,1920,1960,2000]
[null,null,null,null,null,0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26,27,28,29,30,31,32,33,34,35,36,37,38,39,40,41,42,43,44,45,46,47,48,49,50,63]
[]
["4x7bits",28,null,null,"PWMx_WF_Target_Dutycycle"]
[null,null,null,null,null,127]
[]
["4x2x8bits",64,null,null,"PWMx_WF_Fade_Duration",0,40,80,120,160,200,240,280,320,360,400,440,480,520,560,600,640,680,720,760,800,840,880,920,960,1000,1040,1080,1120,1160,1200,1240,1280,1320,1360,1400,1440,1480,1520,1560,1600,1640,1680,1720,1760,1800,1840,1880,1920,1960,2000,2040,2080,2120,2160,2200,2240,2280,2320,2360,2400,2440,2480,2520,2560,2600,2640,2680,2720,2760,2800,2840,2880,2920,2960,3000,3040,3080,3120,3160,3200,3240,3280,3320,3360,3400,3440,3480,3520,3560,3600,3640,3680,3720,3760,3800,3840,3880,3920,3960,4000,4040,4080,4120,4160,4200,4240,4280,4320,4360,4400,4440,4480,4520,4560,4600,4640,4680,4720,4760,4800,4840,4880,4920,4960,5000,5040,5080,5120,5160,5200,5240,5280,5320,5360,5400,5440,5480,5520,5560,5600,5640,5680,5720,5760,5800,5840,5880,5920,5960,6000,6040,6080,6120,6160,6200,6240,6280,6320,6360,6400,6440,6480,6520,6560,6600,6640,6680,6720,6760,6800,6840,6880,6920,6960,7000,7040,7080,7120,7160,7200,7240,7280,7320,7360,7400,7440,7480,7520,7560,7600,7640,7680,7720,7760,7800,7840,7880,7920,7960,8000,8040,8080,8120,8160,8200,8240,8280,8320,8360,8400,8440,8480,8520,8560,8600,8640,8680,8720,8760,8800,8840,8880,8920,8960,9000,9040,9080,9120,9160,9200,9240,9280,9320,9360,9400,9440,9480,9520,9560,9600,9640,9680,9720,9760,9800,9840,9880,9920,9960,10000]
[null,null,null,null,null,0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26,27,28,29,30,31,32,33,34,35,36,37,38,39,40,41,42,43,44,45,46,47,48,49,50,51,52,53,54,55,56,57,58,59,60,61,62,63,64,65,66,67,68,69,70,71,72,73,74,75,76,77,78,79,80,81,82,83,84,85,86,87,88,89,90,91,92,93,94,95,96,97,98,99,100,101,102,103,104,105,106,107,108,109,110,111,112,113,114,115,116,117,118,119,120,121,122,123,124,125,126,127,128,129,130,131,132,133,134,135,136,137,138,139,140,141,142,143,144,145,146,147,148,149,150,151,152,153,154,155,156,157,158,159,160,161,162,163,164,165,166,167,168,169,170,171,172,173,174,175,176,177,178,179,180,181,182,183,184,185,186,187,188,189,190,191,192,193,194,195,196,197,198,199,200,201,202,203,204,205,206,207,208,209,210,211,212,213,214,215,216,217,218,219,220,221,222,223,224,225,226,227,228,229,230,231,232,233,234,235,236,237,238,239,240,241,242,243,244,245,246,247,248,249,250,255]
[]
["4x4bits",16,{"$f":"SUM(B166:B173)","v":28},"Failure","Vf",2.1,2.2000000000000002,2.2999999999999998,2.4,2.5,2.6,2.7,2.8,2.9,3,3.1,3.2,3.3,3.4,3.5,3.6]
[null,null,null,null,null,0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15]
[]
["4x2bits",8,null,null,"LED_Failure_Deact","No_deactivate","Single_Fault","Multiple_Fault"]
[null,null,null,null,null,0,1,2,3]
[]
["4x1bit",4,null,null,"LED_Failure_Report","DISABLE","ENABLE"]
[null,null,null,null,null,0,1]
[]
["Total","bits",{"$f":"SUM(C4:C174)","v":781}]
[null,"byts",{"$f":"ROUNDUP(C175/8,0)","v":98}]

{"sheet":"CHNOutput","index":5,"n_rows":16,"n_cols":6,"rows_kept":16,"cut":false,"hidden":false,"merged":[[7,0,7,1],[7,2,7,3],[15,0,15,4],[4,0,4,1],[4,2,4,3],[5,0,5,1],[5,2,5,3],[6,0,6,1],[6,2,6,3],[0,0,0,3],[1,0,1,3],[2,0,2,1],[2,2,2,3],[3,0,3,1],[3,2,3,3]]}
["CHN Output"]
["CC Output Channel Voltage"]
["Vf_Maximum_voltage(V)",null,50]
["Output Channel ",null,"Function",null,"LED NUM"]
["Channel1",null,"LB",null,7]
["Channel2",null,"HB",null,8]
["Channel3",null,"TI",null,15]
["Channel4",null,"DRL",null,15]
[null,"Function","Duty_Cycle(%)","LSD_CHN_Assign","LED NUM"]
["LSD1","DRL2",20,"Channel4",4]
["LSD2","Not_Used",5,"Not_Used","Not_Used"]
["PWM1","Not_Used",0]
["PWM2","Not_Used",0]
["PWM3","Not_Used",0]
["PWM4","Not_Used",0]
["10100010111010100010011110111111011001010010001000000000101000000000000000000000000000000000000000000000000000",null,null,null,null,{"$f":"LEN(A16)","v":110}]

{"sheet":"HB_TURN_DPL_SBL","index":6,"n_rows":12,"n_cols":12,"rows_kept":12,"cut":false,"hidden":false,"merged":[[2,0,2,1],[3,0,3,1],[4,7,4,8],[11,0,11,4],[4,0,6,0],[0,0,0,2],[0,4,0,5],[0,7,0,8],[0,10,0,11],[1,0,1,1]]}
["HB",null,null,null,"TURN",null,null,"DRL/PO",null,null,"SBL"]
["Ramp_method",null,"BCM_LIN",null,"Signal Source","InputCHN3",null,"Signal Source","BCM_LIN",null," Trigger_SteAngle_Thershold(Deg)",0]
["HB_combined_Front_fog",null,"INVALID",null,"TI_delay_time(ms)",0,null,"DRL_POS_Trigger_Dutycycle(%)","10",null,"Max_Speed_Thershold(Kph)",0]
["LDM_internal_standard_ramping",null,"Immediate",null,null,null,null,"ParkPos_Intensity(%)","5"]
["Fade Speed(ms)","Fast",200,null,null,null,null,"Arbitration"]
[null,"Middle",200,null,null,null,null,"DRL_LB_Outage","No_Impact"]
[null,"Slow",200,null,null,null,null,"DRL_Combined_TI","TI_restrain_DRL/PO"]
[null,null,null,null,null,null,null,"DRL_TI_Control","TI_active,turnoff_DRL1/2orPO2,no_impact_on_PO1"]
[null,null,null,null,null,null,null,"DRL_activation_time_after_deact(ms)",200]
[null,null,null,null,null,null,null,"DRL_ON_FTP","No_Impact"]
[]
["0000000010001000110000100000000010000000001000000000000000000",null,null,null,null,{"$f":"LEN(A12)","v":61}]

{"sheet":"FAN","index":7,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":false,"merged":[[3,0,3,1],[3,2,3,3],[4,0,4,1],[4,2,4,3],[5,0,5,1],[5,2,5,3],[0,0,0,3],[1,0,1,1],[1,2,1,3],[2,0,2,1],[2,2,2,3]]}
["FAN"]
["Activation",null,"LB/HB_Active"]
["NTC",null,"NTC1"]
["Temp(℃）",null,"50"]
["RunTime_OnPwr(s)",null,"0"]
["Outage_Detect",null,"DISABLE"]
["00010000000",{"$f":"LEN(A7)","v":11}]

{"sheet":"BIN","index":8,"n_rows":18,"n_cols":17,"rows_kept":18,"cut":false,"hidden":false,"merged":[[17,0,17,15],[7,1,7,4],[7,5,7,8],[7,9,7,12],[7,13,7,16],[8,2,8,3],[8,6,8,7],[8,10,8,11],[8,14,8,15],[4,0,4,8],[4,9,4,16],[5,0,5,8],[5,9,5,16],[6,0,6,16],[0,0,0,16],[1,0,1,16],[2,0,2,8],[2,9,2,16],[3,0,3,8],[3,9,3,16]]}
["BIN"]
["Channel BIN Source"]
["Channel1",null,null,null,null,null,null,null,null,"BIN_Channel1"]
["Channel2",null,null,null,null,null,null,null,null,"BIN_Channel2"]
["Channel3",null,null,null,null,null,null,null,null,"BIN_Channel3"]
["Channel4",null,null,null,null,null,null,null,null,"BIN_Channel4"]
["BIN LED CHN CFG"]
["Output Channel","Output Channel1",null,null,null,"Output Channel2",null,null,null,"Output Channel3",null,null,null,"Output Channel4"]
["BIN Index","BIN Param Cfg","Resistance level(Ohm)",null,"BIN Current(mA)","BIN Param Cfg","Resistance level(Ohm)",null,"BIN Current(mA)","BIN Param Cfg","Resistance level(Ohm)",null,"BIN Current(mA)","BIN Param Cfg","Resistance level(Ohm)",null,"BIN Current(mA)"]
["BIN0",0,{"$f":"C11","v":900},null,null,0,{"$f":"G11","v":900},null,null,0,{"$f":"K11","v":900},null,null,0,{"$f":"O11","v":900}]
["BIN1",0,{"$f":"IF(B10=0,1000*0.9,590)","v":900},{"$f":"IF(B11=0,1000*1.1,1000+600)","v":1100},850,0,{"$f":"IF(F10=0,1000*0.9,590)","v":900},{"$f":"IF(F11=0,1000*1.1,1000+600)","v":1100},1500,0,{"$f":"IF(J10=0,1000*0.9,590)","v":900},{"$f":"IF(J11=0,1000*1.1,1000+600)","v":1100},260,0,{"$f":"IF(N10=0,1000*0.9,590)","v":900},{"$f":"IF(N11=0,1000*1.1,1000+600)","v":1100},150]
["BIN2",0,{"$f":"IF(B11=0,1800*0.9,1800+200)","v":1620},{"$f":"IF(B12=0,IF(B11=0,1800*1.1,1800+600),1800+1000)","v":1980},850,0,{"$f":"IF(F11=0,1800*0.9,1800+200)","v":1620},{"$f":"IF(F12=0,IF(F11=0,1800*1.1,1800+600),1800+1000)","v":1980},1500,0,{"$f":"IF(J11=0,1800*0.9,1800+200)","v":1620},{"$f":"IF(J12=0,IF(J11=0,1800*1.1,1800+600),1800+1000)","v":1980},260,0,{"$f":"IF(N11=0,1800*0.9,1800+200)","v":1620},{"$f":"IF(N12=0,IF(N11=0,1800*1.1,1800+600),1800+1000)","v":1980},150]
["BIN3",0,{"$f":"IF(B12=0,3160*0.9,3160+200)","v":2844},{"$f":"IF(B13=0,IF(B12=0,3160*1.1,3160+600),3160+1000)","v":3476},850,0,{"$f":"IF(F12=0,3160*0.9,3160+200)","v":2844},{"$f":"IF(F13=0,IF(F12=0,3160*1.1,3160+600),3160+1000)","v":3476},1500,0,{"$f":"IF(J12=0,3160*0.9,3160+200)","v":2844},{"$f":"IF(J13=0,IF(J12=0,3160*1.1,3160+600),3160+1000)","v":3476},260,0,{"$f":"IF(N12=0,3160*0.9,3160+200)","v":2844},{"$f":"IF(N13=0,IF(N12=0,3160*1.1,3160+600),3160+1000)","v":3476},150]
["BIN4",0,{"$f":"IF(B13=0,4870*0.9,4870+200)","v":4383},{"$f":"IF(B14=0,IF(B13=0,4870*1.1,4870+500),4870+1100)","v":5357},850,0,{"$f":"IF(F13=0,4870*0.9,4870+200)","v":4383},{"$f":"IF(F14=0,IF(F13=0,4870*1.1,4870+500),4870+1100)","v":5357},1500,0,{"$f":"IF(J13=0,4870*0.9,4870+200)","v":4383},{"$f":"IF(J14=0,IF(J13=0,4870*1.1,4870+500),4870+1100)","v":5357},260,0,{"$f":"IF(N13=0,4870*0.9,4870+200)","v":4383},{"$f":"IF(N14=0,IF(N13=0,4870*1.1,4870+500),4870+1100)","v":5357},150]
["BIN5",0,{"$f":"IF(B14=0,7150*0.85,7150+0)","v":6077.5},{"$f":"IF(B15=0,IF(B14=0,7150*1.1,7150+700),7150+1500)","v":7865},850,0,{"$f":"IF(F14=0,7150*0.85,7150+0)","v":6077.5},{"$f":"IF(F15=0,IF(F14=0,7150*1.1,7150+700),7150+1500)","v":7865},1500,0,{"$f":"IF(J14=0,7150*0.85,7150+0)","v":6077.5},{"$f":"IF(J15=0,IF(J14=0,7150*1.1,7150+700),7150+1500)","v":7865},260,0,{"$f":"IF(N14=0,7150*0.85,7150+0)","v":6077.5},{"$f":"IF(N15=0,IF(N14=0,7150*1.1,7150+700),7150+1500)","v":7865},150]
["BIN6",0,{"$f":"IF(B15=0,9760*0.91,9760+100)","v":8881.6},{"$f":"IF(B16=0,IF(B15=0,9760*1.05,9760+500),9760+1700)","v":10248},850,0,{"$f":"IF(F15=0,9760*0.91,9760+100)","v":8881.6},{"$f":"IF(F16=0,IF(F15=0,9760*1.05,9760+500),9760+1700)","v":10248},1500,0,{"$f":"IF(J15=0,9760*0.91,9760+100)","v":8881.6},{"$f":"IF(J16=0,IF(J15=0,9760*1.05,9760+500),9760+1700)","v":10248},260,0,{"$f":"IF(N15=0,9760*0.91,9760+100)","v":8881.6},{"$f":"IF(N16=0,IF(N15=0,9760*1.05,9760+500),9760+1700)","v":10248},150]
["BIN7",0,{"$f":"IF(B16=0,13000*0.89,13000+300)","v":11570},{"$f":"IF(B17=0,IF(B16=0,13000*1.1,13000*1.2),13000*1.3)","v":14300},850,0,{"$f":"IF(F16=0,13000*0.89,13000+300)","v":11570},{"$f":"IF(F17=0,IF(F16=0,13000*1.1,13000*1.2),13000*1.3)","v":14300},1500,0,{"$f":"IF(J16=0,13000*0.89,13000+300)","v":11570},{"$f":"IF(J17=0,IF(J16=0,13000*1.1,13000*1.2),13000*1.3)","v":14300},260,0,{"$f":"IF(N16=0,13000*0.89,13000+300)","v":11570},{"$f":"IF(N17=0,IF(N16=0,13000*1.1,13000*1.2),13000*1.3)","v":14300},150]
["000000000001001011010010110100101101001011010010110100101101001011010000000010001100100011001000110010001100100011001000110010001100100000000000010000000100000001000000010000000100000001000000010000110000000000000101000001010000010100000101000001010000010100000101",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"LEN(A18)","v":264}]

{"sheet":"NTC_Derating","index":9,"n_rows":25,"n_cols":13,"rows_kept":25,"cut":false,"hidden":false,"merged":[[24,0,24,7],[14,0,23,0],[14,1,23,8],[6,0,6,4],[6,5,6,8],[7,1,7,2],[7,3,7,4],[7,5,7,6],[7,7,7,8],[3,0,3,4],[3,5,3,8],[4,0,4,4],[4,5,4,8],[5,0,5,4],[5,5,5,8],[0,0,0,8],[1,0,1,4],[1,5,1,8],[2,0,2,4],[2,5,2,8]]}
["NTC"]
["NTC_R0(kΩ)",null,null,null,null,10]
["NTC_B_Constant",null,null,null,null,4000]
["Channel1 NTC Source",null,null,null,null,"NTC1"]
["Channel2 NTC Source",null,null,null,null,"NTC2"]
["Channel3 NTC Source",null,null,null,null,"NTC3"]
["Channel4 NTC Source",null,null,null,null,"NTC4"]
[null,"Output Channel1",null,"Output Channel2",null,"Output Channel3",null,"Output Channel4"]
[null,"Temp(℃）","Dimming(%)","Temp(℃）","Dimming(%)","Temp(℃）","Dimming(%)","Temp(℃）","Dimming(%)"]
["Derate1",-40,0,-40,0,-40,0,-40,0,{"$f":"100-C10","v":100},{"$f":"100-E10","v":100},{"$f":"100-G10","v":100},{"$f":"100-I10","v":100}]
["Derate2",-5,0,-5,0,-5,0,-5,0,{"$f":"100-C11","v":100},{"$f":"100-E11","v":100},{"$f":"100-G11","v":100},{"$f":"100-I11","v":100}]
["Derate3",80,0,80,0,80,0,80,0,{"$f":"100-C12","v":100},{"$f":"100-E12","v":100},{"$f":"100-G12","v":100},{"$f":"100-I12","v":100}]
["Derate4",120,50,120,50,120,50,120,50,{"$f":"100-C13","v":50},{"$f":"100-E13","v":50},{"$f":"100-G13","v":50},{"$f":"100-I13","v":50}]
["Derate5",135,50,135,50,135,50,135,50,{"$f":"100-C14","v":50},{"$f":"100-E14","v":50},{"$f":"100-G14","v":50},{"$f":"100-I14","v":50}]
["Power \nreduction \ncurve"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["10111100000010000000000000110101011101010010000000000000011010101110101001100000000000001101010111010101000000000000000110101011101010",null,null,null,null,null,null,null,{"$f":"LEN(A25)","v":134}]

{"sheet":"Animation","index":10,"n_rows":9,"n_cols":6,"rows_kept":9,"cut":false,"hidden":false,"merged":[[2,1,2,5],[3,1,3,5],[8,0,8,4],[0,0,1,5]]}
["Animation"]
[]
["Welcome_Delay(ms)",1000]
["Farewell_Delay(ms)",1000]
[null,"DRL","PWM1","PWM2","PWM3","PWM4"]
["W/F_Dutycycle(%)",100,0,0,0,0]
["Welcome_Duration(ms)",5000,0,0,0,0]
["Farewell_Duration(ms)",5000,0,0,0,0]
["0110010110011100100011111010111110100000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000",null,null,null,null,{"$f":"LEN(A9)","v":127}]

{"sheet":"LEDFailure","index":11,"n_rows":8,"n_cols":5,"rows_kept":8,"cut":false,"hidden":false,"merged":[[0,0,0,4],[7,0,7,3]]}
["LED_Failure"]
["CHN IDX","CH1","CH2","CH3","CH4"]
["CHN SingleLED Vf(V)",2.2999999999999998,2.2999999999999998,2.2999999999999998,2.2999999999999998]
[]
["FUNC","LB","HB","DRL","TI"]
[" LED_Failure_Deact","No_deactivate","No_deactivate","No_deactivate","No_deactivate"]
[" LED_Failure_Report","ENABLE","ENABLE","ENABLE","ENABLE"]
["0010001000100010001001001001",null,null,null,{"$f":"LEN(A8)","v":28}]